**TEM Protocol**

1. Negative Discharge (Grid treatment) : 45sec
2. In case of salt treatment

* 5uL drop of 1M MgCl2 for 5min, wick off with filter paper

1. U.F. solution treatment:

* 5uL drop of U.F. solution and wick off
* 5uL drop of U.F. solution for 45sec before wicking off

1. Let grid sits for 30min before imaging