


Running buffer in all runs is TEAA 1x 500mM NaCl


Column: KW-803

Pore Size: 100nm









Column: KW-804

Pore Size: 150nm

